{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":5,"rows_kept":8,"merged":[[0,0,1,0],[2,0,3,0],[4,0,5,0],[6,0,7,0]]}
[1,"设备名称","数量","预算单价\n（万）","技术参数"]
[null,"脊柱减压牵引床",1,9.1,"技术参数\n1、牵引模式：连续牵引、三种间歇模式。\n2、实时显示：牵引模式、牵引力、牵引时间、间歇力、间歇时间和总治疗时间\n3、同时进行腰牵和颈牵。\n4、操作显示：触摸控制屏"]
[2,"设备名称","数量","预算单价\n（万）","技术参数"]
[null,"双通道麻醉微量泵",3,0.8,"双通道"]
[3,"设备名称","数量","预算单价\n（万）","技术参数"]
[null,"电火针",1,3.3,"适用于中医针刺治疗"]
[4,"设备名称","数量","预算单价\n（万）","技术参数"]
[null,"射频消融治疗仪",1,9.85,"射频消融仪参数\n1 :基本配置:射频发生器、脚踏开关、电源线。\n2 :射频输出功率： 0-250W±20%；额定负载：50Ω；射频频率：≤475KHz +10%。\n4 :产品温度测量范围：35℃~130℃，根据电极不同温控范围为：55~103℃。\n5: 使用电源：AC220V±22V，50Hz±1Hz；最大供电电流：6.3A。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}